Packaging generating (ECMA standard)

To generate a drawing based on ECMA standard or modify the parameters of the previously generated drawing, select: Edit/Standards/ECMA, press "Alt+E" keys or click button:
Window of packaging parameters will appear. Basic and required parameters are the type of packaging and the 3 basic packaging dimensions. Without them it is not possible to generate the drawing. After selecting the type, will be activated the required fields, while in the lower left corner, example of packaging is displayed. You can move between the different fields by pressing "Tab" key.

In some types of packagings (eg. ECMA A20.20.01.01 AeroplaneTuckEnd) is possible to put an extra locks on the lid. If this option is possible for the current packaging, will activate the option "Lock type". You can choose from 3 options:

- - No lock (default option)
- - Postal lock (safety lock before opening the lid)
- - Thumb cut (Notch allowing easy opening the lid)

To confirm the parameters, click "OK" or press "Enter". If any of the parameters has an invalid value, a window appears with information. To cancel the parameters, click "Cancel" or press "Esc".

Every drawing is generated on the layer "1 sample - bottom". If the packaging is made up of 2 parts (bottom and lid) then drawing will appear also on the layer "1 sample - lid".