File

To create a new project, select: File/New, press "Ctrl+N" keys or click button:
You can create more than one project and work on several projects at the same time. Change the active project by selecting the interesting item from menu: Window/"Filename" or pressing "Ctrl+Tab" or "Ctrl+Shift+Tab" keys.

To save the project, select: File/Save, press "Ctrl+S" keys or click button:

To save the project under a different name or in a different location, select: File/Save As or press "Ctrl+Shift+S" keys.

To open a previously saved project, select: File/Open, press "Ctrl+O" keys or click button:

To open the project saved in a different format (import it) select: File/Import, press "Ctrl+I" keys or click button:
Is possible to import from a format:

- AutoCad Interchange (*.DXF)
- CFF2 (*.CF2)

To create a new project (or several projects) based on text file (batch processing) choose: File/New based on file or press "Ctrl+Shift+N" keys
Program creates one or more projects and exports as .dxf to the directory, from which text file was read
Example commands:

- queryno: LetterBottom
- template: FEFCO 0215
- flute: B
- thickness: 2,8
- length: 200
- width: 100
- height: 150,50
- Layout: Yes
- sheetWidth: 2000
- sheetHeight: 1200
- sheetMarginBottom: 20
- sheetMarginTopMin: 10
- sheetMarginLeftMin: 10
- sheetMarginRightMin: 10
- queryno: DoubleWallsTray
- template: FEFCO 0425
- flute: B
- thickness: 3
- length: 300,00
- width: 220,5
- height: 51
- queryno: TelescopeBottomLid
- template: FEFCO 0330
- flute: E
- thickness: 1,5
- length: 250,00
- width: 180
- height: 60
- Layout: 1
- sheetWidth: 1600
- sheetHeight: 1100
- sheetMarginBottom: 22
- sheetMarginTopMin: 15
- sheetMarginLeftMin: 5
- sheetMarginRightMin: 5
- LidLayout: true
- LidsheetWidth: 1600
- LidsheetHeight: 1100
- LidsheetMarginBottom: 22
- LidsheetMarginTopMin: 15
- LidsheetMarginLeftMin: 5
- LidsheetMarginRightMin: 5
- Command: "queryno" is query name and filename at once.
- Command: "Layout" or "LidLayout" lets to optimal arrange units on the sheet. Required value: yes, 1 or true

To save the project in a different format (export it) select: File/Export, press "Ctrl+E" keys or click button:
The project can be exported to a format:

- AutoCad Interchange (*.DXF)
- CFF2 (*.CF2)
- HPGL (*.HPG)
- CNC Machine Tool Path (*.NC)
- Scalable Vector Graphics (*.SVG)

To print the current layer, select: File/Print, press "Ctrl+P" keys or click button:
Layer that is currently displayed on the screen will be printed. The drawing is scaled so that was visible the entire display area. So if, for example, on the screen on the left and the right background areas are free, they are also taken into account in the calculation of the optimal scale of the printed drawing.

To print the current layer in the scale of 1:1, select: File/Print 1:1 scale, press "Ctrl+Shift+P" keys or click button:
Layer that is currently displayed on the screen will be printed in the scale 1:1. If the sheet of the printer is less than the current layer, you will see the central section only. This feature is useful when printing a drawing on large-format printing plotters.